Alokasi Frekuensi 2.3 – 2.45 GHz

Onno W. Purbo

Menurut Draft KEPMEN Alokasi Frekuensi 	2.3 – 2.45GHz di Indonesia (region 3 ITU) di peruntukan:

1.	Servis Tetap (fix wireless)
2.	Servis Bergerak (mobile wireless)
3.	Amatir Radio
4.	Radiolokasi (radio locator)

Penggunaannya mengacu kepada ITU

S5.150
S5.282
S5.393
S5.394
S5.396

Detail dari pasal-pasal ITU S5 tsb adalah sbb:

S5.43 (1)
Jika ditandai di dalam Regulasi ini bahwa dinas dapat beroperasi pada pita frekuensi tertentu dengan tanpa menyebabkan "harmful interference", hal ini berarti bahwa dinas tersebut tidak dapat mengajukan proteksi dari "harmful interference" yang disebabkan oleh dinas lain pada pita yang dialokasikan di bawah Bab SII dari Radio Regulations.

S5.150	
The following bands:
13 553 - 13 567 kHz	(centre frequency 13 560 kHz),
26 957 - 27 283 kHz	(centre frequency 27 120 kHz),
40.66 - 40.70 MHz	(centre frequency 40.68 MHz),
902 - 928 MHz	in Region 2 (centre frequency 915 MHz),
2 400 - 2 500 MHz	(centre frequency 2 450 MHz),
5 725 - 5 875 MHz	(centre frequency 5 800 MHz), and
24 - 24.25 GHz	(centre frequency 24.125 GHz)
are also designated for industrial, scientific and medical (ISM) applications. Radiocommunication services operating within these bands must accept harmful interference which may be caused by these applications. ISM equipment operating in these bands is subject to the provisions of No. S15.13.

S5.282	
In the bands 435 - 438 MHz, 1 260 - 1 270 MHz, 2 400 - 2 450 MHz, 3 400 - 3 410 MHz (in Regions 2 and 3 only) and 5 650 - 5 670 MHz, the amateur-satellite service may operate subject to not causing harmful interference to other services operating in accordance with the Table (see No. S5.43). Administrations authorizing such use shall ensure that any harmful interference caused by emissions from a station in the amateur-satellite service is immediately eliminated in accordance with the provisions of No. S25.11. The use of the bands 1 260 - 1 270 MHz and 5 650 ? 5 670 MHz by the amateur-satellite service is limited to the Earth-to-space direction.
S5.393	
Additional allocation:  in the United States, India and Mexico, the band 2 310-2 360 MHz is also allocated to the broadcasting-satellite service (sound) and complementary terrestrial sound broadcasting service on a primary basis. Such use is limited to digital audio broadcasting and is subject to the provisions of Resolution 528 (WARC-92).      (WRC-97)

S5.394
In the United States, the use of the band 2 300 - 2 390 MHz by the aeronautical mobile service for telemetry has priority over other uses by the mobile services. In Canada, the use of the band 2 300 - 2 483.5 MHz by the aeronautical mobile service for telemetry has priority over other uses by the mobile services.

S5.396
Space stations of the broadcasting-satellite service in the band 2 310 ? 2 360 MHz operating in accordance with No. S5.393 that may affect the services to which this band is allocated in other countries shall be coordinated and notified in accordance with Resolution 33. Complementary terrestrial broadcasting stations shall be subject to bilateral coordination with neighbouring countries prior to their bringing into use.